**Command Line Arguments**

Both the server and client are invoked through the command line arguments

The P2MP-FTP server is invoked as follows:

p2mpserver port# file-name p

where port# is the port number to which the server is listening (for this project, this port number is always 7735), file-name is the name of the file where the data will be written, and p is the packet loss probability.

The P2MP-FTP client must be invoked as follows:

p2mpclient server-1 server-2 server-3 server-port# file-name MSS

where server-i is the host name where the i-th server (receiver) runs, i = 1, 2, 3, server-port# is the port number of the server (i.e., 7735), file-name is the name of the file to be transferred, and MSS is the maximum segment size.